***Flammable and combustible liquids***

2.10.2.3. **Flammable** **liquids** and **combustible liquids** shall be stored in conformance with Part 4 and in areas inaccessible to children.

Subsection 2.10.3. Staffing

2.10.3.1. Where children with disabilities are cared for, sufficient staff shall be present at all times during the period the children are in the centre to escort them to safety in the event of a fire emergency.

***Flammable and combustible liquids***

5.14.9.6. The storage, handling and use of **flammable** **liquids** and **combustible liquids** shall meet the requirements of Part 4.

5.14.9.7. (1) During the pin refinishing process, a receptacle that complies with Sentence 2.4.1.3.(3) shall be provided for waste rags and materials used in operations involving flammable finishes or solvents.

(2) The contents of each receptacle referred to in Sentence (1) shall be removed daily and disposed of in an **approved** manner.

Subsection 5.14.10. Drycleaning and Dyeing Plants

***Application***

5.14.10.1. (1) Drycleaning plants shall comply with NFPA 32, “Standard for Drycleaning Plants”.

(2) Despite Sentence (1) and subject to Article 5.14.10.2., **flammable liquids**shall not be used for any purpose in drycleaning and dyeing plants.

***Use and storage of flammable liquids***

5.14.10.2. (1) **Flammable liquids** may be used as a local application to remove spots and stains if the liquids

(a) are stored in containers that have a capacity of not more than 1 L,

(b) do not exceed more than 25 L in aggregate quantity, and

(c) are dispensed from plastic containers that have a capacity of not more than 0.5 L.

(2) Despite Sentence (1), existing drycleaning plants and dyeing plants may be **approved** if the **Chief Fire Official** is satisfied that the level of fire safety specified in Sentence (1) is provided.